**Facility Status Definitions**

* **Immediate** pertains to work that is emergency in nature. The Work Package may be developed in parallel to doing this type of work (see section 3.1.8 Immediate Work) and indicating this category on the Work requests permits tracking and reporting of these events
* **Anytime** means the work can occur at any time regardless of beam status.
* **Partial Outage** means the beam must be off in some areas but it is not required to be shut down completely. There are different categories for:

**Partial Outage Accelerator/Target**

 **Partial Outage Neutron Instruments**

* **Maintenance Day** means the work requires the beam to be shut down completely but can reasonably occur within the period of one day (the Maintenance Day).
* **Planned Outage** means the work requires the beam to be shut down for an extended period, typically the Summer or Winter major outages, to accomplish the full scope of the work.
* .